{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":105,"n_cols":11,"rows_kept":105,"merged":[[0,0,0,10],[2,0,4,0],[2,2,4,2],[5,0,9,0],[5,2,9,2],[10,0,15,0],[10,2,15,2],[16,0,23,0],[16,2,23,2],[24,0,41,0],[24,2,41,2],[42,0,51,0],[42,2,51,2],[52,0,59,0],[52,2,59,2],[60,0,80,0],[60,2,80,2],[81,0,92,0],[81,2,92,2],[93,0,103,0],[93,2,103,2],[104,1,104,8]]}
["01包段广宣项目门窗清单"]
["序号","标段","位置","序号","清单名称","清单特征","单位","工程量","含税单价（元）","合价（元）","备注"]
[1,"标段1","广德服务区",1,"普通铝合金门连窗 ","1、玻璃品种、厚度：门窗玻璃采用铝合金推拉窗5高透Low-E+19Ar(百叶)+5暖边\n2、外门窗框料采用普通铝合金。","m2",61.86]
[null,"标段1",null,2,"铝合金推拉窗 ","1、玻璃品种、厚度：5mm厚钢化玻璃\n2、所有窗户均需外设金刚纱纱窗","m2",32.94]
[null,"标段1",null,3,"断热铝合金窗 ","1、玻璃品种、厚度：6mm普通钢化白玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",71.64]
[2,"标段2","绿锦服务区",4,"普通铝合金推拉门 ","1、外门窗框料采用普通铝合金。","m2",100.8]
[null,"标段2",null,5,"断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：断热铝合金窗5中透光Low--E+12氩气+5,自身遮阳系数0.65\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",891.29]
[null,"标段2",null,6,"断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：铝合金外窗5高透Low-E+19Ar(百叶)+5暖边,夏季遮阳系数0.27,传热系数2.1W/m2·K\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",891.29]
[null,"标段2",null,7,"玻璃门 ","1、玻璃品种、厚度：玻璃门","m2",10.8]
[null,"标段2",null,8,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：6+12A+6遮阳型\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",53.64]
[3,"标段3","洪林服务区",9,"普通铝合金推拉门 ","1、外门窗框料采用普通铝合金。","m2",252]
[null,"标段3",null,10,"断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：断热铝合金窗5中透光Low--E+12氩气+5,自身遮阳系数0.65\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",866.635]
[null,"标段3",null,11,"断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：铝合金外窗5高透Low-E+19Ar(百叶)+5暖边,夏季遮阳系数0.27,传热系数2.1W/m2·K\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",866.635]
[null,"标段3",null,12,"金属门 ","1、门名称、代号及洞口尺寸：超白长虹玻璃移门\n2、门材质：超厚超窄钛镁铝合金型材边框","m2",184.26]
[null,"标段3",null,13,"玻璃门 ","1、玻璃品种、厚度：玻璃门","m2",8.1]
[null,"标段3",null,14,"断热铝合金窗 ","1、玻璃品种、厚度：6mm普通钢化白玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",143.28]
[4,"标段4","洪林收费站",15,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",51.68]
[null,"标段4",null,16,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",90.86]
[null,"标段4",null,17,"80系断热铝合金平开窗（中透光玻璃） ","1、玻璃品种、厚度：5中透光Low-E+9氩气+5\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",82.29]
[null,"标段4",null,18,"断热铝合金自动密闭平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",26.856]
[null,"标段4",null,19,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",152.064]
[null,"标段4",null,20,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",51.408]
[null,"标段4",null,21,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",264.816]
[null,"标段4",null,22,"断热铝合金窗 ","1、玻璃品种、厚度：10厚蓝灰色钢化玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",34.2]
[5,"标段5","十字收费站、十字养护工区、广德西",23,"断热铝合金自动密闭平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",26.856]
[null,"标段5",null,24,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",152.064]
[null,"标段5",null,25,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",51.408]
[null,"标段5",null,26,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",264.816]
[null,"标段5",null,27,"断热铝合金窗 ","1、玻璃品种、厚度：10厚蓝灰色钢化玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",34.2]
[null,"标段5",null,28,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",51.68]
[null,"标段5",null,29,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",173.15]
[null,"标段5",null,30,"铝合金窗（高透光玻璃） ","1、窗材质：普通铝合金，窗用主型材基材壁厚外窗不小于1.8\n2、玻璃品种、厚度：门窗玻璃采用金属隔热型材隔热条高度26mm(K=2.8)5高透Low-E+19Ar(百叶)+5暖边(K=2.2)\n3、外门窗开启扇设置纱窗扇\n4、含消防救援窗","套",8]
[null,"标段5",null,31,"断热铝合金平开门 ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边","m2",29.55]
[null,"标段5",null,32,"金属窗  ","1、窗材质：断热铝合金玻璃窗\n2、玻璃品种、厚度：6+12A+6\n3、五金：包含全套五金配件\n4、其他：其他未尽事宜详见图纸、答疑及相关规范要求","m2",123.53]
[null,"标段5",null,33,"金属窗  ","1、窗材质：80系列普通铝合金推拉窗\n2、玻璃品种、厚度：PT90TLC（钢化玻璃 6Low-E+12A+6）(P34-∆P3-q16-K5) GB/T8478","m2",227.59]
[null,"标段5",null,34,"推拉平开门 ","1、窗材质：铝合金玻璃门\n2、玻璃品种、厚度：6+12A+6\n3、五金：包含全套五金配件\n4、其他：其他未尽事宜详见图纸、答疑及相关规范要求","m2",68.06]
[null,"标段5",null,35,"金属门 ","1、部位：卫生间门\n2、门材质：铝合金玻璃门；\n3、玻璃品种、厚度：钢化玻璃\n4、五金：包含全套五金配件\n5、其他未尽事宜详见图纸、答疑及相关规范要求","m2",18.48]
[null,"标段5",null,36,"金属窗 ","1、窗材质：普通铝合金，窗用主型材基材壁厚外窗不小于1.8\n2、玻璃品种、厚度：门窗玻璃采用金属隔热型材隔热条高度26mm(K=2.8)5高透Low-E+19Ar(百叶)+5暖边(K=2.2)\n3、外门窗开启扇设置纱窗扇\n4、含消防救援窗","m2",108.21]
[null,"标段5",null,37,"金属门 ","1、门材质：铝合金外门主型材厚度不应小于2mm\n2、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",5.75]
[null,"标段5",null,38,"金属门 ","1、部位：厨房门\n2、门材质：铝合金玻璃门；\n3、玻璃品种、厚度：钢化玻璃\n4、五金：包含全套五金配件\n5、其他未尽事宜详见图纸、答疑及相关规范要求","m2",5.13]
[null,"标段5",null,39,"铝合金窗（高透光玻璃） ","1、窗材质：普通铝合金，窗用主型材基材壁厚外窗不小于1.8\n2、玻璃品种、厚度：门窗玻璃采用金属隔热型材隔热条高度26mm(K=2.8)5高透Low-E+19Ar(百叶)+5暖边(K=2.2)\n3、外门窗开启扇设置纱窗扇\n4、含消防救援窗","套",60]
[null,"标段5",null,40,"铝合金窗（高透光玻璃） ","1、窗材质：普通铝合金，窗用主型材基材壁厚外窗不小于1.8\n2、玻璃品种、厚度：门窗玻璃采用金属隔热型材隔热条高度26mm(K=2.8)5高透Low-E+19Ar(百叶)+5暖边(K=2.2)\n3、外门窗开启扇设置纱窗扇\n4、含消防救援窗","套",10]
[6,"标段6","高湖收费站",41,"断热铝合金自动密闭平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",26.856]
[null,"标段6",null,42,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",152.064]
[null,"标段6",null,43,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",51.408]
[null,"标段6",null,44,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",264.816]
[null,"标段6",null,45,"断热铝合金窗 ","1、玻璃品种、厚度：10厚蓝灰色钢化玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",34.2]
[null,"标段6",null,46,"断热铝合金平开门（高透光玻璃）） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",51.68]
[null,"标段6",null,47,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",90.86]
[null,"标段6",null,48,"80系断热铝合金平开窗（中透光玻璃） ","1、玻璃品种、厚度：5中透光Low-E+9氩气+5\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",82.29]
[null,"标段6",null,49,"断热铝合金平开门 ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边","m2",13.44]
[null,"标段6",null,50,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：6中透光Low-E+12氩气+6透明/5高透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇\n3、含消防救援窗","m2",84.3]
[7,"标段7","宣城东收费站",51,"断热铝合金自动密闭平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",40.508]
[null,"标段7",null,52,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",166.81]
[null,"标段7",null,53,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",55.875]
[null,"标段7",null,54,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",250.214]
[null,"标段7",null,55,"断热铝合金窗 ","1、玻璃品种、厚度：10厚蓝灰色钢化玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",21.24]
[null,"标段7",null,56,"定制铝合金门 ","1、门材质：定制铝合金门（含门套）\n2、其他：含内置隔音棉、不锈钢合页、不锈钢执手锁、不锈钢门吸，静音密封条，挂衣钩，成品门套等一切五金配件\n3、所有门尺寸需现场复核\n4、说明：包含门洞上楣装饰板包边，清单工程量按门洞面积计量，投标人综合考虑报价","m2",20.74]
[null,"标段7",null,57,"卫生间铝合金门 ","1、门名称、代号及洞口尺寸：卫生间铝合金门","樘",6]
[null,"标段7",null,58,"卫生间铝合金门 ","1、门名称、代号及洞口尺寸：卫生间铝合金门","樘",12]
[8,"标段8","宣城西收费站",59,"断热铝合金窗 ","1、玻璃品种、厚度：10厚蓝灰色钢化玻璃\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",21.24]
[null,"标段8",null,60,"卫生间成品隔断 ","1、隔断材料品种、规格：18mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",55.44]
[null,"标段8",null,61,"卫生间铝合金门 ","1、门名称、代号及洞口尺寸：卫生间铝合金门","樘",8]
[null,"标段8",null,62,"铝合金窗（高透光玻璃） ","1、窗材质：普通铝合金，窗用主型材基材壁厚外窗不小于1.8\n2、玻璃品种、厚度：门窗玻璃采用金属隔热型材隔热条高度26mm(K=2.8)5高透Low-E+19Ar(百叶)+5暖边(K=2.2)\n3、外门窗开启扇设置纱窗扇\n4、含消防救援窗","套",60]
[null,"标段8",null,63,"断热铝合金自动密闭平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",23.076]
[null,"标段8",null,64,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",304.128]
[null,"标段8",null,65,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",98.28]
[null,"标段8",null,66,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",464.832]
[null,"标段8",null,67,"铝合金门 ","门材质：铝合金门","m2",31.28]
[null,"标段8",null,68,"断热铝合金组合窗 ","1、玻璃品种、厚度：断热铝合金组合窗\n2、含消防救援窗\n3、所有窗户均需外设金刚纱纱窗","m2",44.07]
[null,"标段8",null,69,"定制铝合金门 ","1、门材质：定制铝合金门（含门套）\n2、其他：含内置隔音棉、不锈钢合页、不锈钢执手锁、不锈钢门吸，静音密封条，挂衣钩，成品门套等一切五金配件\n3、所有门尺寸需现场复核\n4、说明：包含门洞上楣装饰板包边，清单工程量按门洞面积计量，投标人综合考虑报价","m2",23.79]
[null,"标段8",null,70,"断热铝合金平开门（高透光玻璃）） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",15.95]
[null,"标段8",null,71,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",7.2]
[null,"标段8",null,72,"断热铝合金平开门（高透光玻璃）） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",33.84]
[null,"标段8",null,73,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",130.5]
[null,"标段8",null,74,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",26.56]
[null,"标段8",null,75,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",163.48]
[null,"标段8",null,76,"铝合金窗 ","1、窗名称：铝合金窗\n2、玻璃品种、厚度：高透Low-E+19Ar(百叶)+5暖边）\n3、配成品带纱扇\n4、未尽事宜：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","m2",142.2]
[null,"标段8",null,77,"普通铝合金窗 ","1、窗名称：普通铝合金窗\n2、配成品带纱扇\n3、未尽事宜：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","m2",15.36]
[null,"标段8",null,78,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",45.18]
[null,"标段8",null,79,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",660.72]
[9,"标段9","广德东、广德改造收费站",80,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",51.68]
[null,"标段9",null,81,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",173.15]
[null,"标段9",null,82,"断热铝合金自动密闭平开门（高透光玻璃）） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",29.23]
[null,"标段9",null,83,"断热铝合金推拉门 ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边","m2",157.594]
[null,"标段9",null,84,"金属门 ","1、门名称、代号及洞口尺寸：详见图纸\n2、门材质：6厚磨砂玻璃塑钢玻璃门","m2",52.668]
[null,"标段9",null,85,"断热铝合金推拉窗 ","1、窗代号及洞口尺寸：详见图纸\n2、窗材质：5高透Low-E+19Ar（百叶）+5暖边\n3、玻璃品种：断热铝合金推拉窗","m2",260.194]
[null,"标段9",null,86,"断热铝合金平开门（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",73.32]
[null,"标段9",null,87,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",207.21]
[null,"标段9",null,88,"断热铝合金平开门（高透光玻璃）） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含350mm高护门板\n3、含横执把手","m2",26.56]
[null,"标段9",null,89,"80系断热铝合金平开窗（高透光玻璃） ","1、玻璃品种、厚度：5高透Low-E+19Ar(百叶)+5暖边\n2、含金刚纱纱窗\n3、含消防救援窗\n4、含手动开启装置","m2",163.48]
[null,"标段9",null,90,"铝合金推拉窗 ","1、玻璃品种、厚度：5mm厚钢化玻璃\n2、所有窗户均需外设金刚纱纱窗","m2",33.12]
[null,"标段9",null,91,"卫生间铝合金门 ","1、门名称、代号及洞口尺寸：卫生间铝合金门","樘",12]
[10,"标段12",null,92,"金属门 ","1、自动密闭铝合金平开门\n2、门名称、代号及洞口尺寸：LM1021\n3、玻璃：12厚钢化玻璃\n4、包含所有五金配件","m2",12]
[null,"标段12",null,93,"断热铝合金平开门 ","1、玻璃品种、厚度：5中透Low-E+9 氩气+5","m2",88.8]
[null,"标段12",null,94,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",306.18]
[null,"标段12",null,95,"断热铝合金平开门 ","1、玻璃品种、厚度：5中透Low-E+9 氩气+5","m2",20.91]
[null,"标段12",null,96,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",2.88]
[null,"标段12",null,97,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",41.37]
[null,"标段12",null,98,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",18.36]
[null,"标段12",null,99,"断热铝合金平开门 ","1、玻璃品种、厚度：5中透Low-E+9 氩气+5","m2",20.91]
[null,"标段12",null,100,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",2.88]
[null,"标段12",null,101,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",41.37]
[null,"标段12",null,102,"80系列断热铝合金窗（中透光玻璃） ","1、玻璃品种、厚度：5中透Low-E+19Ar(百叶)+5暖边\n2、外门窗开启扇设置纱窗扇","m2",18.36]
[11,"总计",{"$nulls":7},{"$f":"SUM(J3:J104)","v":{"v":0,"d":"0.00"}}]