{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["采购清单","品牌推荐表"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"采购清单","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"merged":[[0,0,0,7],[2,2,4,2],[6,1,6,4],[7,0,7,6],[8,0,8,6]]}
["G3京台高速公路蚌埠互通至路口枢纽改扩建工程木门采购清单"]
["序号","门名称","项目特征","单位","数量","单价（元）","合价（元）","备注（注明品牌）"]
[1,"单开门","1.门名称：实木复合烤漆门（含门套）\n2.门材质：科技木皮门烤漆门（含门套）\n3.（1）门扇厚度≥45mm\n  （2）门扇表层贴科技木皮烤漆饰面，基层为不低于8mm厚热压多层板（或欧松板、密度板）；门芯部分由实木方料填芯（杉木、松木，禁用回收旧料）或桥洞力学板；\n  （3）门套采用不低于22mm厚多层板（或欧松板、密度板）、门套线条为60mm宽全木线条，表层贴科技木皮烤漆饰面，底部背面做防潮处理；\n  （4）科技木皮选用厚度不低于28S，颜色秋木浅麦，饰面颜色、花纹以设计选样确定为准；\n4.五金品种、规格：门扇合页4*3*2不锈钢，机械50大锁体、（尺寸按实际选样确定）；\n5.五金品牌：坚朗、顶固、名门、尼克、汇泰龙、海诗蔓、美国MOOTO、梓德；\n6．其他：含内置隔音棉、不锈钢合页、不锈钢执手锁、不锈钢门吸，静音密封条，挂衣钩，成品门套等一切五金配件；\n7．说明：包含门洞上楣装饰板包边，清单工程量按土建洞口面积计量，投标人综合考虑报价；\n8.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求。","m2",1300]
[2,"第三卫生间单开门",null,"m2",15]
[3,"双开门",null,"m2",143]
[4,"门楣板","门楣板板材为9mm厚密度板，表面贴科技木皮烤漆饰面，两侧门套线到顶，门套线不计入门楣板面积。","m2",40]
[5,"合计"]
["1、增值税税率13%，含人工、材料、机械、运输装卸、安装、检测验收、成品保护、垃圾清运等全部费用"]
["2、以上单价为固定单价，乙方应综合考虑各类风险，中标后，不得以任何理由要求调价或补偿费用。"]

{"sheet":"品牌推荐表","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}