{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"merged":[[0,0,0,7],[9,0,9,5]],"flags":["formulas_cached_only"]}
["          铝合金门窗采购清单                                    "]
["序号","名称",null,"单位","数量","单价（元）","小计（元）","备注\n（注明品牌）"]
[1,"百叶窗","1、铝合金防雨百叶窗\n2、厚度：壁厚0.8mm\n3、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n4、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",21.24]
[2,"普通铝合金窗","1、窗材质90型断桥铝（壁厚1.8mm）。\n2、玻璃品种、厚度：6高透双银low-e+12Ar+6玻璃、\n3、外开窗纱一体隔热条高度34mm  自身遮阳系数0.46，传热系数1.8，二层玻璃\n4、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n5、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",35.67]
[3,"平开窗","1、玻璃品种、厚度：6高透双银low-e+12Ar+6玻璃，\n2、铝合金门窗用主型材基材壁厚：窗材质90型断桥铝（壁厚1.8mm）\n3、外开窗纱一体，隔热条高度34mm  自身遮阳系数0.46，传热系数1.8，二层玻璃\n4、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n5、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",425.28]
[4,"下悬窗","1、玻璃品种、厚度：6高透双银low-e+12Ar+6玻璃，\n2、铝合金门窗用主型材基材壁厚：窗材质90型断桥铝（壁厚1.8mm）\n3、外开窗纱一体，隔热条高度34mm  自身遮阳系数0.46，传热系数1.8，二层玻璃\n4、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n5、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",13.5]
[5,"消防窗","1、玻璃品种、厚度：6高透双银low-e+12Ar+6玻璃、\n2、铝合金门窗用主型材基材壁厚：窗材质90型断桥铝（壁厚1.8mm）\n3、外开窗纱一体，隔热条高度34mm  自身遮阳系数0.46，传热系数1.8，二层玻璃\n4、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n5、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",31.2]
[6,"推拉门","1、玻璃品种、厚度：铝合金推拉门，8mm厚的安全玻璃\n2、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n3、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",138]
[7,"平开门","1、玻璃品种、厚度：6高透双银low-e+12Ar+6玻璃\n2、铝合金门窗用主型材基材壁厚：窗材质120型断桥铝（壁厚1.8mm）\n3、外开窗纱一体，隔热条高度34mm  自身遮阳系数0.46  传热系数1.8，二层玻璃\n4、五金材料、品种、规格：五金配件齐全（含一切相关辅材）及墙内外接缝打胶\n5、具体做法：详见图纸、图集、答疑、招标文件、政府相关文件、规范等其他资料，满足验收要求","㎡",46.06]
["合计"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}