{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":7,"rows_kept":6,"merged":[[0,0,0,6],[5,0,5,4]]}
["太蕲木门清单明细"]
["门名称","项目特征","数量","单位","单价（元)","小计（元)","备注（品牌）"]
["免漆单扇门","1.门名称：免漆单扇门（含门套）\n2.门材质：PVC覆膜（含门套）\n3.（1）桥动力学板条间隔3—5公分填充；门套基层:12mm厚细木工板点状打底\n  （2）门扇表层面做单色PVC覆膜，\n  （3）门扇厚度大于等于45mm，其中标准为:5.7mm密度板（0.16mmpvc覆膜）、33mmLVL边框档和33mm复合龙骨桥洞力学板填充；\n  （4）成品门套板:双层5.7mm密度板、12mm多层板/实木板、0.16mmpvc覆膜\n4.五金品种、规格：门扇合页4*3*2不锈钢，（尺寸按实际选样确定）；\n5.五金品牌：梓德、坚朗、顶固、名门、汇泰龙、海诗、尼克；                                                6.其他：配套门锁、合页、不锈钢门吸，挂衣钩，成品门套等一切五金配件；\n7.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求。",{"$f":"[1]Sheet1!$C$3*[1]Sheet1!$C$4+[1]Sheet1!$C$6+[1]Sheet1!$C$7","v":1038},"㎡"]
["免漆单扇门","1.门名称：免漆单扇门（含门套）（内木门，具有烟密闭性能和自动关闭功能）\n2.门材质：:PVC覆膜（含门套）\n3.（1）桥动力学板条间隔3—5公分填充；门套基层:12mm厚细木工板点状打底\n  （2）门扇厚度大于等于45mm，其中标准为:5.7mm密度板（0.16mmpvc覆膜）、33mmLVL边框档和33mm复合龙骨桥洞力学板填充\n  （3）成品门套板:双层5.7mm密度板、12mm多层板/实木板、0.16mmpvc覆膜\n  （4）成品门套线:50mm宽pvc覆膜门套线条；\n4.五金品牌：梓德、坚朗、顶固、名门、汇泰龙、海诗、尼克；\n5．其他：不锈钢合页、不锈钢执手锁、不锈钢门吸，挂衣钩，成品门套等一切五金配件；\n6.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求。",{"$f":"[1]Sheet1!$C$5","v":69},"㎡"]
["免漆双扇门","1.门名称：免漆双扇门（含门套）\n2.门材质：:PVC覆膜，双开开门（含门套）\n3.（1）内部填充：桥动力学板条间隔3—5公分填充；门套基层:12mm厚细木工板点状打底\n  （2）门扇厚度大于等于45mm，其中标准为:5.7mm密度板（0.16mmpvc覆膜）、33mmLVL边框档和33mm复合龙骨桥洞力学板填充\n  （3）.成品门套板:双层5.7mm密度板、12mm多层板/实木板、0.16mmpvc覆膜\n  （4）成品门套线:50mm宽pvc覆膜门套线条；\n4.五金品牌：梓德、坚朗、顶固、名门、汇泰龙、海诗、尼克；\n5.其他：不锈钢合页、不锈钢执手锁、不锈钢门吸，挂衣钩，成品门套等一切五金配件；\n6.具体详见图纸、图集、答疑、招标文件、政府相关文件、规范等其它资料，满足验收要求。",{"$f":"[1]Sheet1!$C$8+[1]Sheet1!$C$9","v":10},"㎡"]
["合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}