{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"merged":[[0,0,0,7],[2,7,13,7],[14,0,14,5]]}
["03包段合肥至周口高速公路颍上（南照）至临泉（皖豫界）段房建项目"]
["序号","清单名称","清单特征","单位","工程量","单价（含税13%）","合价（元）","备注"]
[1,"卫生间成品隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",380,null,null,"1.采用覆膜工艺；\n2.面层厚度为0.6mm；\n3.铝蜂窝芯孔径为8mm*8mm；\n4.五金均选用304不锈钢材质；\n5.报价含税费、运费、检测复试费等相关费用"]
[2,"卫生间小便器隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",7.54]
[3,"卫生间成品隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",380]
[4,"卫生间小便器隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",7.54]
[5,"卫生间成品隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",455]
[6,"卫生间小便器隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",7.54]
[7,"卫生间成品隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",455]
[8,"卫生间小便器隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",7.54]
[9,"卫生间成品隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",476]
[10,"卫生间小便器隔断","1、隔断材料品种、规格：20mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",8.88]
[11,"卫生间成品隔断","1、隔断材料品种、规格：18mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口，不锈钢门铰，不锈钢衣钩，不锈钢抽手，不锈钢门锁，有无人指示灯等配件","m2",476]
[12,"卫生间小便器隔断","1、隔断材料品种、规格：18mm原木纹蜂窝铝板\n2、配件品种、规格：含不锈钢收口等配件","m2",8.88]
["合计"]