{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["东区","西区"],"not_rendered":{"images":6},"read":"whole","date_system":"1900"}

{"sheet":"东区","index":0,"n_rows":13,"n_cols":10,"rows_kept":13,"merged":[[0,0,0,9],[2,7,4,7],[8,7,10,7],[11,1,11,5],[12,0,12,9]]}
["陈埠服务区东区幕墙铝单板采购项目\n"]
["序号","名称","规格参数","单位","数量","综合单价\n（元）","合价（元）","铝板样式参考图片","品牌","使用部位"]
[1,"幕墙铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",3313.17,{"$nulls":4},"檐口及包柱"]
[2,"幕墙圆弧单曲铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",1000,{"$nulls":4},"檐口及包柱"]
[3,"幕墙双曲铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",150,{"$nulls":4},"檐口及包柱"]
[4,"幕墙铝单板","3mm厚深灰色氟碳油漆喷涂","㎡",91.12,{"$nulls":4},"幕墙墙面"]
[5,"幕墙铝单板","3mm厚浅灰色氟碳油漆喷涂","㎡",1843.85,{"$nulls":4},"幕墙墙面"]
[6,"幕墙穿孔铝单板","3mm厚木色（香槟色）氟碳油漆喷涂","㎡",1288.47,{"$nulls":4},"女儿墙"]
[7,"室内吊顶铝单板","3mm厚白色氟碳油漆喷涂","㎡",250,{"$nulls":4},"室内顶面及柱面"]
[8,"室内吊顶圆弧单曲铝单板","3mm厚白色氟碳油漆喷涂","㎡",800,{"$nulls":4},"室内顶面及柱面"]
[9,"室内吊顶双曲铝单板","3mm厚白色氟碳油漆喷涂","㎡",250,{"$nulls":4},"室内顶面及柱面"]
[10,"合计"]
["报价说明：\n1.二次图纸深化设计及现场尺寸测量、排版下料费用、下料损耗等含在综合单价里。                                                            2.铝单板按设计图示尺寸以展开面积计算，折边隐藏进行固定部分，面积不在另计算。\n3.供应商应充分熟悉图纸及现场情况，后期不能以铝单板造型复杂，如超宽超长、圆弧焊接刨槽等情况要求增加费用。"]

{"sheet":"西区","index":1,"n_rows":13,"n_cols":9,"rows_kept":13,"merged":[[0,0,0,8],[2,7,4,7],[8,7,10,7],[11,1,11,5],[12,0,12,8]]}
["陈埠服务区西区幕墙铝单板采购项目\n"]
["序号","名称","规格参数","单位","数量","综合单价\n（元）","合价（元）","铝板样式参考图片","使用部位"]
[1,"幕墙铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",3313.17,{"$nulls":3},"檐口及包柱"]
[2,"幕墙圆弧单曲铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",1000,{"$nulls":3},"檐口及包柱"]
[3,"幕墙双曲铝单板","3mm厚银灰色氟碳油漆喷涂","㎡",150,{"$nulls":3},"檐口及包柱"]
[4,"幕墙铝单板","3mm厚深灰色氟碳油漆喷涂","㎡",91.12,{"$nulls":3},"幕墙墙面"]
[5,"幕墙铝单板","3mm厚浅灰色氟碳油漆喷涂","㎡",1843.85,{"$nulls":3},"幕墙墙面"]
[6,"幕墙穿孔铝单板","3mm厚木色（香槟色）氟碳油漆喷涂","㎡",1288.47,{"$nulls":3},"女儿墙"]
[7,"室内吊顶铝单板","3mm厚白色氟碳油漆喷涂","㎡",250,{"$nulls":3},"室内顶面及柱面"]
[8,"室内吊顶圆弧单曲铝单板","3mm厚白色氟碳油漆喷涂","㎡",800,{"$nulls":3},"室内顶面及柱面"]
[9,"室内吊顶双曲铝单板","3mm厚白色氟碳油漆喷涂","㎡",250,{"$nulls":3},"室内顶面及柱面"]
[10,"合计"]
["报价说明：\n1.二次图纸深化设计及现场尺寸测量、排版下料费用、下料损耗等含在综合单价里。                                                            2.铝单板按设计图示尺寸以展开面积计算，折边隐藏进行固定部分，面积不在另计算。\n3.供应商应充分熟悉图纸及现场情况，后期不能以铝单板造型复杂，如超宽超长、圆弧焊接刨槽等情况要求增加费用。\n"]